**Steps for replacing anode**


1. Remove cover



1. Disconnect hose from cold water inlet elbow



1. Remove cold water inlet elbow





1. Remove anode

